Input will always be of the form {Left Sensor, Front Sensor, Right Sensor}

* There are four possibilities with regards to orientation \*\ We can set states or if statements
* Micromouse is facing forward
* Micromouse is facing backwards
* Micromuse is to the left
* Micromuse is to the right